{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["店招类室外广告报价单"],"not_rendered":{"external_links":2,"defined_names":12},"read":"whole","date_system":"1900"}

{"sheet":"店招类室外广告报价单","index":0,"n_rows":24,"n_cols":8,"rows_kept":24,"merged":[[0,0,0,7],[2,0,6,0],[7,0,17,0],[10,2,11,2],[18,0,21,0],[22,0,23,0],[28,0,28,4],[29,0,29,4],[30,0,30,4],[31,0,31,4]]}
["店招及灯箱物料清单（初拟）"]
[" 类别","序号","项目","工艺规格材质","备注或详细说明","单位","保修期","年度需求数量"]
["店招类制作         ",1,"单面喷绘布店招-计展开面积  （无包边条，不打灯）","内部框架及支架：宽2.5x2.5cm壁厚1.0mm镀锌方管焊接，支架含一般支架：特殊支架另外计价\n固定用螺丝：膨胀螺丝 \n\n","喷绘布材料：520内打或外打光灯布；灯布品牌：无要求；喷绘机：无要求；喷绘精度：400dpi ，喷绘精度如进口机按400dpi 国产机需500dpi以上\n","平米","一年"]
[null,2,"箱体式喷绘布店招-计正面及两侧面面积             （无包边条，不打灯）","内部框架：宽2.5x2.5cm厚1.2mm方管焊接或3*3cm角钢厚2mm\n背封：0.3mm厚镀锌铁皮; 固定用螺丝：膨胀螺丝","喷绘布材料：520内打或外打光灯布；灯布品牌：无要求；喷绘机：无要求；喷绘精度：400dpi ，喷绘精度如进口机按400dpi 国产机需501dpi以上\n","平米","一年"]
[null,3,"铝塑板店招-计展开面积（不打灯）","箱体 + 铝塑板面板（亚克力立体雕刻字或发光字价格另计，见下述配件）","箱体框架：宽4x2.0cm厚1.2mm镀锌扁管焊接，铝塑板品牌：吉祥；板材厚度：3mm厚。","平米","一年"]
[null,4,"烤漆扣板店招—计展开面积（不打灯）","箱体 + 烤漆扣板（亚克力立体雕刻字或吸塑字价格另计，见下述配件）；","箱体框架：宽4x2.0cm厚1.2mm镀锌扁管焊接，烤漆三维扣板或是条状扣板","平米","一年"]
[null,5,"大方板板店招—计展开面积（不打灯）","箱体 + 大方板（亚克力立体雕刻字或吸塑字价格另计，见下述配件）；","箱体框架：宽4x2.0cm厚1.2mm镀锌扁管焊接，烤漆三维扣板或是条状扣板","平米","一年"]
["店招及灯箱类配件                ",6,"喷绘布换画面","喷绘布材料：520内打或外打光灯布；灯布品牌：无要求；喷绘机：无要求；喷绘精度：400dpi","喷绘精度如进口机按400dpi 国产机需500dpi以上","平米","一年"]
[null,7,"包边条 （按店招或灯箱平米数计价）","包边材料：0.6mm~0.8mm厚不锈铁或钛金 规格：1+3+4或1+3+5",null,"平米","一年"]
[null,8,"内置灯管","灯管：40W 整流器：2根灯管配一个 无品牌要求，2根灯管加一个整流器为一套","注：为保证亮度，每平方米需配四根灯管，即两套","套","一年"]
[null,9,"外打射灯","高度小于5M: 250W外打灯射灯（带变压器）品牌：不限     ","支架和护导线","套","一年"]
[null,10,null,"高度大于5M: 400W外打灯射灯（带变压器）品牌：不限     ","支架和护导线","套","一年"]
[null,11,"彩钢瓦","厚：0.3mm，无品牌要求",null,"平方米","一年"]
[null,12,"烤漆字","0.5mm厚锌铁皮烤漆，按字体图形切割平面，侧面宽3~4cm锌铁皮烤漆围边","如面积小于1平米，按最长边*1计算面积，如果面积大于1平米，按实际长宽计算面积","平米","一年"]
[null,13,"亚克力发光字","亚克力面板厚度：3mm-5mm 直角围边0.4mm 铝塑围边","LED模块：每个模块3个灯点，单个灯点亮度0.024W，12伏变压器，白光灯；（如面积小于1平米，按最长边*1计算面积，如果面积大于1平米，按实际长宽计算面积）\n","平米","一年"]
[null,14,"外露灯发光字","镀锌面板雕刻+镀锌围边+烤漆，外露灯发光字厚度：5~8CM","LED模块：每个模块4个灯点，单个灯点亮度0.024W，12伏变压器，白光灯；（如面积小于1平米，按最长边*1计算面积，如果面积大于1平米，按实际长宽计算面积）\n","平米","一年"]
[null,15,"pvc字","2cm厚pvc字；大于等于25cm高","需喷漆","平米","一年"]
[null,16,"pvc字","2cm厚pvc字；低于25cm高","需喷漆","个","一年"]
["灯具类                   ",17,"数码管","半圆型多彩数码管，8CM-10CM",null,"米","一年"]
[null,18,"灯带","每米计算 多彩或单彩",null,"米","一年"]
[null,19,"日光灯","40w  灯管  无品牌要求 ",null,"支","一年"]
[null,20,"吊顶筒灯（含节能灯）","25w  无品牌要求",null,"个","一年"]
["灯箱类制作             ",21,"角铁灯箱-计正面面积                            （如为移动灯箱滑轮价格另计）","灯箱厚度:25-30cm，内部框架：宽2.5*2.5cm或3*3cm，厚1.5mm方管焊接\n或：宽3*3cm厚2mm或宽4*4cm厚3mm角铁焊接                                                                            ","喷绘布材料：520打光灯布\n喷绘机：无要求\n喷绘精度：400dpi\n灯管：无\n","平米","一年"]
[null,22,"超薄灯箱（铝型材框架）","灯箱厚度：10cm\n内部框架及支架：宽2.5x2.5cm厚1.2mm镀锌方管焊接（焊接点防锈处理）\n内衬：厚3mm乳白色有机玻璃\n表面：厚5mm有机玻璃（中间写真灯片）                                                                                                                                  包边材料：0.8mm厚不锈钢（喷漆）\n包边规格：宽3+2cm                                                                                                                                               四周封边：0.4mm厚铝塑板\n背封：0.4mm厚镀锌板\n固定用螺丝：膨胀螺丝","写真灯片：720DPI；灯管：36W飞利浦T5灯管\n镇流器：飞利浦镇流器\n灯管配置：每平米4套；每个灯箱独立电源开关","平米","一年"]